
# Imaging Setup Checklist

* Turn on lightbox and camera
* Remove lens cap
* Set focus mode to AF (autofocus)
* Create new folder on desktop
* Obtain specimens (fill out cabinet log)
* Start imaging log entry
* Open Smart Shooter 3
* Connect camera
* Check settings (they should match below)



* Set image directory to your new folder
* Set name policy to [S]

**Now you’re ready to (1) load your first specimen, (2) set the focal point, and (3) start imaging!**

*Make sure you set the focus to manual (M) on the camera once you have set your focal point!*